# Clifton Cameras Product Specification

## Hawke Frontier ED X 10x32 Binoculars

## Imaging

**Power:** 10×

**Objective:** 32mm

**Lens Coating:** Fully Multi-Coated (FMC)

**Field of View:** m @1000m / ft @1000yds 108m / 324ft

**Close Focus:** 3m / 9.8ft

**Eye relief:** 15mm / 0.6″

**Exit Pupil:** 3.2mm / 0.13″

**Prism Type:** Dielectric Mirror Coating

**Interpupillary Distance:** 56-74mm / 2.2-2.9″

**Dioptre System:** Right Eye

## General

**Dimensions:** 120mm x 118mm

**Weight:** 540g / 19oz

**Eyecups:** Twist-Up

**Warranty:** Hawke Worldwide Warranty

Nitrogen Purged, Waterproof and Fog Proof

## Accessories

Instruction Manual, Quality Assurance Booklet, Lens Cloth, Protective Case, Case Strap, Harness Adaptors, Neck Strap, Objective Lens Covers, Ocular Lens Covers