# Clifton Cameras Product Specification

## Fujifilm XF 80mm F2.8 R LM OIS WR Fujinon Macro Lens Full Spec

**Type**

FUJINON LENS XF80mmF2.8 R LM OISWR Macro

**Lens construction**

16 elements 12 groups

(includes 1 aspherical , 3ED and 1 super ED elements）

**Focal length (35mm format equivalent)**

f=80mm (122mm)

**Angle of view**

20.1°

**Max. aperture**

F2.8

**Min. aperture**

F22

**Aperture control**

**Number of blades**

9（rounded diaphragm opening）

**stop size**

1/3EV (19 steps)

**Focus range**

25cm～∞

**Max. magnification**

1x

**External dimensions: Diameter x Length (approx.)（distance from camera lens mount flange）**

Φ80mm x 130mm

**Weight (approx.) (excluding caps, hoods ）**

750g

**Filter size**

Φ62mm

**Accessories included**

Lens cap FLCP-62Ⅱ

Lens rear cap RLCP-001

Lens hood

Lens pouch